Logical Interconnect Groups > Create a logical interconnect group |  | next

# Create a logical interconnect group

By default, a single logical interconnect group containing all the interconnects in the enclosure is automatically created when you add an enclosure. If you want to create multiple logical interconnects, create the logical interconnect groups first with the interconnects you want in each logical interconnect. See About multiple logical interconnect groups in an enclosure group and When to create a logical interconnect group for more information.

If you want to use an existing logical interconnect group as a template, copy the logical interconnect group rather than create a new one.

Prerequisites

- Required privileges: Network administrator or Infrastructure administrator

Creating a logical interconnect group

1. From the main menu, select Logical Interconnect Groups, and then do one of the following:

   - Select Actions→Create.

   - Click + Create logical interconnect group.

2. Enter a name for the logical interconnect group.

3. Select from the list of available interconnects for each bay. See Logical interconnect group requirements for more information.

4. Click the Edit icon of the internal network area in the graphical view.

5. Click Add networks to select from available networks.

6. Click OK when you are finished adding the internal networks.

7. Click Add uplink set.

8. Enter the data requested on the screen for each uplink set you want to create. See Add an uplink set for more information.

9. Click Create to finish, or click Create + to create additional uplink sets.

10. Optional: Scroll down and, if necessary, make changes to the interconnect settings.

    Any logical interconnects created from the interconnect group inherit these settings. For more information, see Interconnect settings.

11. Optional: Make any changes to the SNMP settings.

    Any logical interconnects created from the interconnect group inherit these settings. For more information, see SNMP.

12. Optional: Make any changes to the Quality of Service (QoS) settings.

13. Click Create to finish, or click Create + to create additional logical interconnect groups.

14. To verify that the logical interconnect group was created, locate the group in the details pane.

15. Optional: Select the logical interconnect group to edit, and then select Actions→Edit to make changes to the utilization sampling settings, if necessary.

    These settings are used in data collection for the utilization graphs displayed on the Interconnects screen. For more information, see Utilization Sampling.

16. Click OK to apply any changes.

17. To verify the changes, locate them in the General view.

### More information

About logical interconnect groups
Return to Quick Start: Initial configuration of resources in HPE OneView

prev | up | next
Logical Interconnect Groups screen details | home | Edit a logical interconnect group

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP