Logical Interconnects > Read a logical interconnect MAC address table |  | next

# Read a logical interconnect MAC address table

The MAC address table can be used to troubleshoot your network. The table includes information to help you identify the associated networks, uplink sets, and server profiles. You can get up to a maximum of 100 entries per `GET` operation.

### Prerequisites

- Minimum required session ID privileges: Infrastructure administrator or Network administrator

Reading a logical interconnect MAC address table using REST APIs
Select the logical interconnect URI. `GET /rest/logical-interconnects` Get the logical interconnect MAC address table. `GET `{logical interconnect URI}`/forwarding-information-base`

prev | up | next
Find noncompliant logical interconnects | home | Read the internal networks in a logical interconnect

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP