Firmware > Upload a firmware bundle |  | next

# Upload a firmware bundle

Update the firmware repository on the appliance by uploading a firmware bundle, also known as a Service Pack for ProLiant (SPP). An SPP is a comprehensive update package of firmware, drivers, and utilities delivered as a single PXE-bootable ISO image. After the firmware bundle has been uploaded to the repository, it can be set as the firmware baseline for one device or across a set of devices. Firmware baselines for servers are managed using server profiles, either by editing an existing server profile or by creating a new server profile to include a new service pack. To manage firmware baselines for enclosures and interconnects, edit a device configuration directly.

### Prerequisites

- Minimum required session ID privileges: Infrastructure administrator, Server administrator, or Network administrator

Uploading a firmware bundle using REST APIs
`POST /rest/firmware-bundles`

See also

- Quick Start: Initial configuration using REST APIs

prev | up | next
Update enclosure firmware | home | Upload a hotfix

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP