Logical Switches > Edit a logical switch |  | next

# Edit a logical switch

A maximum of two switches is allowed. If there is only one switch, you can edit switch data and add a second switch. If there are two switches, you can delete one of them. Additionally, the operational mode of the logical switch can be changed between `Monitored` and `Managed`.

| NOTE: Editing a logical switch can make it inconsistent with its logical switch group. To make the logical switch consistent, update the logical switch from the logical switch group.

## Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

## Editing a logical switch

1. From the main menu, select Logical Switches.

2. In the master pane, select the logical switch that you want to edit and select Actions→Edit.

3. Edit the values shown on the screen.

4. Confirm your changes, and click OK to apply them.

5. Verify that the changes appear in the details pane.

prev | up | next
Create a logical switch | home | Change logical switch operational mode

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP