Interconnects > Clearing port counters |  | next

# Clearing port counters

After you configure an interconnect, the appliance can capture statistics about network traffic on the interconnect ports and subports including transmit, receive, and error counters. Port counters are not available for the Virtual Connect 8Gb 20-port Fibre Channel Module.

The Clear port counters feature resets the port counters to 0 (zero) and records a reset for the collection period. This clears all ports on the interconnect.

## Prerequisites

- Minimum required privileges: Infrastructure administrator or Network administrator

- The interconnect is managed

## Clearing port counters

1. From the main menu, select Interconnects.

2. In the master pane, select the interconnect.

3. Select Actions→Clear port counters.

   | NOTE: The Clear port counters action starts immediately, confirmation is not required.

4. If the activity is successful, the activity displays a green status in the Notifications area. If not, follow the proposed resolution listed under Details in the Notifications area.

prev | up | next
Add an interconnect | home | Enable or disable uplink or downlink ports on an interconnect

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP