Enclosures > About VCM settings that will not be migrated |  | next

# About VCM settings that will not be migrated

The following VCM settings will not be migrated into HPE OneView.

- User account specific information such as certificates, user accounts, LDAP, RADIUS, TACACS+, session timeout, and user role configurations

- Port monitoring configuration. After migration, port monitoring can be configured separately on each logical interconnect. See Configure a port to monitor network traffic for more information.

- Address pools of MACs, WWNs, and serial numbers defined in VCM. HPE OneView migrates the MACs, WWNs, and serial numbers that are part of assigned profiles.

  | NOTE: Any new addresses allocated in HPE OneView after the migration are pulled from the HPE OneView address pools. An administrator can manually define custom ranges in HPE OneView to match those that were defined in VCM to continue allocating from that range.

prev | up | next
About migrating partially stacked domains | home | Before migrating c7000 enclosures

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP