Settings: Appliance Networking > Configure the appliance network at first-time login |  | next

# Configure the appliance network at first-time login

The first time you log in to the appliance as `administrator`, you are instructed to configure the appliance network. However, if you are logging in from the console, you do not need to enter the networking configuration data.

Prerequisites

- You have gathered the information you need to configure the appliance network, as described in Add or edit networking panel screen details.

- Ensure that the tasks for adding enclosures have completed.

- Ensure that the tasks for forming a high availability cluster have completed.

Configuring the appliance network

1. Enter the appliance network configuration information described in Add or edit networking panel screen details.

2. Click OK to configure the network.

   A security warning is displayed. Click Proceed Anyway.

See also

- Quick Start: Initial configuration of HPE OneView

- Settings: Appliance Networking

prev | up | next
Change to a dual-stack protocol | home | Ping a host name or IP address

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP