Logical Interconnects > Edit internal networks |  | next

# Edit internal networks

You can add or remove internal networks from the Logical Interconnects or Logical Interconnect Groups screen. The internal network configuration created in the logical interconnect group is inherited by associated logical interconnects. A logical interconnect can be made consistent with the parent logical interconnect group by selecting Actions→Update from group.

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Editing internal networks

1. From the main menu, select Logical Interconnects, and then select the logical interconnect to edit.

2. Select Actions→Edit.

3. Click the Edit icon of the internal network area in the graphical view.

4. Click Add networks to select from available networks, click Remove All to remove all networks, or click to delete a specific network.

   Make the appropriate changes. See Internal Networks for more information.

   | NOTE: Removing an Ethernet network from an uplink set in a logical interconnect automatically moves it to internal networks so network connectivity is not lost for server profile connections using the network. However, if you remove an Ethernet network from an uplink set in a logical interconnect group, the network does not get moved automatically to the internal networks.

5. Click OK when you are finished editing the internal networks.

6. Check the confirmation box, confirming you understand the presented implications of the action.

7. Click Yes, perform action to continue.

8. Click OK when you are finished editing the logical interconnect.

9. Verify your changes in the Internal Networks view.

### More information

About internal networks

prev | up | next
Edit uplink sets | home | Manage redistribution login settings for uplink failover on a Fibre Channel network

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP