Understanding the security features of HPE OneView > Authentication for appliance access |  | next

# Authentication for appliance access

Access to the appliance requires authentication using a user name and password. User accounts are configured on the appliance or in an enterprise directory. All access (browser and REST APIs), including authentication, occurs over SSL to protect the credentials during transmission over the network.

prev | up | next
Creating a login session | home | Controlling access for authorized users

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP