Logical Interconnect Groups > Edit a logical interconnect group |  | next

# Edit a logical interconnect group

You can edit the following information in a logical interconnect group:

- Add another physical interconnect (or remove existing)

- Change the type of interconnect

- Edit uplink sets by selecting or deselecting uplink ports, adjusting port speeds, and selecting preferred ports

- Add networks to uplink sets and internal networks

- Edit interconnect settings

- Edit utilization sampling rates

- Manage the frequency of control messages through the LACP timer

- Edit Quality of Service (QoS) settings

Any changes are applied to the logical interconnects when a logical enclosure is created or updated from its enclosure group.

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Editing a logical interconnect group

1. From the main menu, select Logical Interconnect Groups and select the interconnect group to edit.

2. Select Actions→Edit.

3. Make your changes in the logical interconnect group to the interconnect configuration, internal networks, associated uplink sets, interconnect settings, or utilization sampling rates.

   | NOTE: Follow the Logical interconnect group requirements when adding or changing interconnects.

4. Click OK.

5. Verify your changes by selecting the appropriate views. For example, if you changed interconnect settings, select the Interconnect settings view for the logical interconnect group to view your changes.

6. To have your changes take effect on logical interconnects that already exist, you can go to the logical interconnect and select Update from group, or go to the logical enclosure associated with the logical interconnect and select Update from group.

See also

- Logical Interconnect Groups

prev | up | next
Create a logical interconnect group | home | Delete a logical interconnect group

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP