Logical Interconnects > Reapply the logical interconnect configuration to its physical interconnects |  | next

# Reapply the logical interconnect configuration to its physical interconnects

You can reapply the logical interconnect configuration to all physical interconnects associated with the logical interconnect when they are not consistent. For example, if you replace a failed physical interconnect you can reapply the logical interconnect configuration. This brings the physical interconnect into consistency with the network connection properties defined by the logical interconnect.

Prerequisites

- Required privileges: Network administrator or Infrastructure administrator

Reapplying the logical interconnect configuration

1. From the main menu, select Logical Interconnects, and then select the logical interconnect.

2. Select Actions→Reapply configuration.

3. Click Yes, reapply to confirm.

4. To verify that the activity is successful, check the activity for a green status in the Notifications area.

   If the activity is not successful, follow the instructions in the proposed resolution.

prev | up | next
Manage the frequency of control messages through the LACP timer | home | Update firmware for logical interconnects within enclosures

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP