Enclosures > Reapply the enclosure configuration |  | next

# Reapply the enclosure configuration

For c7000 enclosures, the Reapply Configuration action re-runs the OA configuration script associated with the logical enclosure. The action also verifies that SSO, SNMP and NTP are configured correctly on the enclosure and that the OA firmware is up to date. If connectivity has been lost to the enclosure, you are prompted to re-enter the OA IP address or host name and credentials.

| NOTE: You cannot reapply an enclosure configuration to monitored enclosures.

Prerequisites

- Required privileges: Infrastructure administrator or Server administrator

Reapplying the configuration

1. From the main menu, select Enclosures.

2. In the master pane, select the enclosure to which you want to reapply the configuration.

3. Select Actions→Reapply Configuration.

4. Click OK.

5. To verify that the activity is successful, check the activity for a green status in the Notifications area.

   If the activity is not successful, follow the instructions in the proposed resolution.

See also

- Enclosures (top of chapter)

prev | up | next
Prepare a VCEM enclosure for migration into HPE OneView | home | Refresh the enclosure to re-synchronize it with HPE OneView

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP