Logical Interconnects > Edit a logical interconnect |  | next

# Edit a logical interconnect

You can edit the following information of a logical interconnect. If you want to change interconnect types, see Edit a logical interconnect group.

- Add or remove networks to and from internal networks

- Add, edit, or remove uplink sets

- Edit interconnect settings

- Edit SNMP settings

  Edit utilization sampling rates

Any changes are applied to the logical interconnects when a logical enclosure is created or updated from its enclosure group.

| NOTE: If a server has connections that use this logical interconnect, editing the logical interconnect might disrupt network connectivity for those servers. For example, updating firmware or changing an uplink set containing networks used by connections defined in the server profile could disrupt connectivity.

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Editing a logical interconnect

1. From the main menu, select Logical Interconnects, and then select the interconnect group to edit.

2. Select Actions→Edit.

3. Make your changes to the logical interconnect. See Logical Interconnects screen details for more information.

4. Click OK.

5. Verify your changes by selecting the appropriate view. For example, if you changed interconnect settings, select the Interconnect settings view.

6. To have your changes take effect on logical interconnects that already exist, you can go to the logical interconnect and select Update from group, or go to the logical enclosure associated with the logical interconnect and select Update from group.

prev | up | next
Delete an uplink set | home | Edit uplink sets

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP