Logical Interconnects > About the Virtual Connect FlexFabric–20/40 F8 interconnect module |  | next

# About the Virtual Connect FlexFabric–20/40 F8 interconnect module

The Virtual Connect FlexFabric–20/40 F8 Module for HPE BladeSystem c-Class has several unique features. For more information, see the HPE Virtual Connect FlexFabric–20/40 F8 Module for HPE BladeSystem c-Class Installation Instructions at http://www.hpe.com/info/qs.

### Enclosure requirements

| CAUTION: To avoid overheating: Make sure there are 10 fans in the enclosure. Do not insert more than six Virtual Connect FlexFabric–20/40 F8 modules in one enclosure.

prev | up | next
About SNMP settings | home | Create an uplink set

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP