Logical Interconnects > Edit uplink sets |  | next

# Edit uplink sets

The Edit screen provides a graphical view of the logical interconnect and its stacking links and uplink sets. Use this screen to make the following configuration changes to a logical interconnect:

- Add uplink sets.

- Edit uplink sets (select or deselect uplink ports, adjust port speed, select preferred ports).

- Add or remove a network to an uplink set.

- Edit the LACP timer.

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Editing the uplinks of a logical interconnect

1. From the main menu, select Logical Interconnects, and then select the logical interconnect to edit.

   | NOTE: If the uplink set contains uplink ports from multiple interconnects, you cannot add FCoE networks.

2. Select Actions→Edit.

3. Click the Edit icon of the uplink set in the graphical view.

4. Make the appropriate changes. See Create or edit uplink sets for more information.

   | NOTE: Any networks removed from uplink sets are automatically added to the internal networks.

5. Click OK.

6. Verify your uplink set changes in the Uplink Sets view.

More information

- Logical Interconnects

prev | up | next
Edit a logical interconnect | home | Edit internal networks

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP