Enclosures > Effects of managing a c7000 enclosure |  | next

# Effects of managing a c7000 enclosure

When an enclosure is being managed by HPE OneView, the following enclosure settings are in effect:

- A management account is created.

- SNMP is enabled and the appliance is added as an SNMP trap destination.

- NTP (Network Time Protocol) is enabled and the appliance becomes the NTP time source.

- The NTP default polling interval is set to 8 hours.

- An appliance certificate is installed to enable single sign-on operations.

- Enclosure firmware management is disabled (except for monitored enclosures).

- Virtual Connect Manager is disabled on the Virtual Connect interconnects in this enclosure.

- The Onboard Administrator (OA) firmware is updated to minimum firmware levels, listed in the HPE OneView Support Matrix (except for monitored enclosures).

See also

- Enclosures

prev | up | next
Prerequisites for bringing a c7000 enclosure into HPE OneView | home | Enclosures screen details

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP