Logical Enclosures > Update firmware from a logical enclosure |  | next

# Update firmware from a logical enclosure

You can update firmware from a logical enclosure for shared infrastructure, shared infrastructure and profiles, and OA (Onboard Administrators) only, if any.

Prerequisites

- Required privileges: Infrastructure administrator or Server administrator

- One or more SPPs are added to the appliance firmware repository.

- Power off any servers that do not have profiles.

Updating firmware from a logical enclosure

1. From the main menu, select Logical Enclosures.

2. In the master pane, select the enclosure on which you want to update a firmware bundle.

3. Select Actions→Update firmware.

4. Enter the data requested on the screen.

5. Click OK.

   As the update progresses, if any one component of the update fails, the logical enclosure update will fail.

6. Verify that the new firmware baseline is listed in the details pane of the Logical Enclosures screen.

##### More information

About updating firmware from a logical enclosure
Firmware Bundles

prev | up | next
Update the logical enclosure configuration from the enclosure group | home | Bring an unmanaged enclosure with invalid firmware under management

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP