Logical Interconnects > Manage SNMP access for c7000 enclosures |  | next

# Manage SNMP access for c7000 enclosures

- Add access for an SNMP manager

- Edit access for an SNMP manager

- Remove access from an SNMP manager

## Add access for an SNMP manager

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

- Not available for Virtual Connect Fibre Channel interconnects

Adding access for an SNMP manager

1. From the main menu, select Logical Interconnects or Logical Interconnect Groups, select the logical interconnect, and then do one of the following:

   - Select Actions→Edit.

   - Click the Edit icon.

2. In the SNMP view, click Add SNMP access.

3. Enter the IP address or subnet of the SNMP manager.

   | NOTE: Both IPv4 and IPv6 addresses are supported.

4. Click Add, or click Add + to add access to other SNMP managers.

5. Click OK.

6. To verify that the specified SNMP access was added, locate the SNMP access information in the SNMP view.

## Edit access for an SNMP manager

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Editing access for an SNMP manager

1. From the main menu, select Logical Interconnects or Logical Interconnect Groups, select the logical interconnect, and then do one of the following:

   - Select Actions→Edit.

   - Click the Edit icon.

2. In the SNMP view, click the Edit icon in the SNMP access row for the address to edit.

3. Make any changes to the IP address.

   | NOTE: Both IPv4 and IPv6 addresses are supported.

4. Click OK to apply your changes.

5. Click OK.

6. To verify that the specified SNMP access was changed, locate the SNMP access information in the SNMP view.

## Remove access from an SNMP manager

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Removing access for an SNMP manager

1. From the main menu, select Logical Interconnects or Logical Interconnect Groups, select the logical interconnect, and then do one of the following:

   - Select Actions→Edit.

   - Click the Edit icon.

2. In the SNMP view, click the Delete icon in the SNMP access row for the address to remove.

3. Click Yes, remove to confirm the deletion.

4. Click OK.

5. To verify that the specified SNMP access was removed, make sure the access no longer displays in the SNMP view.

See also

- Logical Interconnects (top of chapter)

- Logical Interconnect Groups (top of chapter)

prev | up | next
Manage redistribution login settings for uplink failover on a Fibre Channel network | home | Manage SNMP trap destinations

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP