Logical Interconnects > Add an uplink set |  | next

# Add an uplink set

Each uplink set must have a unique name within the logical interconnect or logical interconnect group and contain at least one network. For more information about uplink sets, see About logical interconnects.

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Adding an uplink set

1. From the main menu, select Logical Interconnects, and then select the logical interconnect to edit.

2. Select Actions→Edit.

3. Click the Add uplink set button.

4. Enter the data requested on the screen. See Create or edit uplink sets for more information.

5. Click Add networks and select the networks to assign to the uplink set.

6. Click Add, or click Add + to add another network.

7. Click Add uplink ports and select the uplink ports.

8. Click Add, or click Add + to add another port.

9. Confirm the information you are entering is correct and click Create.

10. Click OK.

11. Verify that the uplink set was created in the details pane.

More information

- Logical Interconnects

prev | up | next
Logical Interconnects screen details | home | Configure a port to monitor network traffic

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP