Server Hardware > Server Hardware screen details |  | next

# Server Hardware screen details

- Overview

- Hardware

- Firmware

- Ports

- Remote Support

- Add Server Hardware

- Edit a rack server

## Overview

#### Utilization panel

The appliance gathers utilization data on various metrics and displays them in the Utilization panel and the Utilization screen

If your server hardware has an iLO advance license, the appliance collects data on the following metrics:

- CPU utilization

- Power consumption (Average, Peak, and Power cap)

- Temperature

In the Utilization panel, the utilization meters depict the portion of the available capacity of the metric utilized during the most recent five-minute data collection period.

Hover your pointer over a meter to see a graph of the metric over the last 24 hours.

Click a meter to go to the Utilization screen to view utilization graphs.

| NOTE: There are some cases where the Utilization panel does not display utilization data. Data is only collected when the server is powered on. See About the Utilization panel for more information.

#### Activities panel

The activities panel shows the three most recent alerts and tasks, in order of severity. You can click any of the severity icons to view alerts for server hardware with that severity. Click More to view all server hardware activities.

#### More information

Utilization screen details
Standard UI buttons
Labels screen details
Map view screen details
Server Hardware

## Hardware

#### State

State of the server hardware such as `Profile Applied`, `No Profile Applied`, or `Unmanaged`.

See Server Hardware states for more information.

#### Server profile

Enables you to view the server profile assigned to the server, and facilitates creating and adding a server profile if the server does not have one.

Use the server profile hyperlink to see the server profile assigned to the server. Use the add server profile hyperlink to navigate to the page for defining a profile.

Once a profile is applied you will also see the health state.

#### Server power

Power status (on or off) of the server

#### Model

Model, which is the same as the product name (for example, ProLiant BL460c Gen8)

#### Server hardware type

The server hardware type of this server. Server hardware types enable you to assign server profiles to hardware based on a certain server hardware type.

#### Product ID

Identification number of the server model

#### Serial number

Factory serial number of the server

#### License

The license type applied to the server hardware.

#### UUID

The universally unique identifier (UUID) for server hardware

#### iLO

The host name, IPv4, and IPv6 addresses for the server iLO.

Clicking on one of the hyperlinks will take you to the iLO web UI.

#### Location

Enclosure and bay number for the server. The enclosure is a hyperlink to the Enclosures screen. The rack is a hyperlink to the Racks screen.

#### Powered by

Power delivery device or devices that are connected to the server hardware

#### Asset tag

Identifies hardware for tracking and inventory purposes

#### Maximum power

The maximum power the device can consume in watts

#### CPU

CPU type and speed

#### Memory

Amount of memory

#### ROM Version

Version of the server firmware or rack server firmware

#### iLO version

Version of the installed iLO firmware

#### Intelligent Provisioning version

Version of the HPE Intelligent Provisioning firmware on the server

#### More information

About licensing
About server hardware types
Icon descriptions

## Firmware

A message is displayed only when the server is powered off. The current inventory will be displayed after the server is powered on.

#### Component

The name of the component for which the firmware version displays.

| NOTE: The location of the devices are displayed in gray.

#### Installed

The version of firmware installed on the component.

| NOTE: If the iLO firmware version is below 2.30, only iLO, ROM, and intelligent provisioning versions are displayed. The versions that cannot be read from server hardware display as `unknown`. When the option card does not support UEFI protocol, the version display as `unknown`. For Gen 8 servers when Agentless Management Service (AMS) is not installed, the version display as `unknown`. The firmware versions on hardware components that do not have UEFI-compatible firmware and Management Component Transport Protocol (MCTP) support display as `unknown`. System ROM installed firmware version must be at least one version greater than or equal to the version that is available in the Service Pack for ProLiant (SPP) 2015.10.0 (applies only for Gen 8 servers). Agentless Management Service (AMS) must be installed to get the complete inventory of the server. When the iLO firmware is updated outside of HPE OneView, a server hardware refresh is required to update the current firmware inventory.

## Ports

Lists information about each adapter on the server, where the adapter is located in the server, the ports on each adapter, and what interconnect each port is connected to.

#### Slot

Displays information about optional hardware that is added to the server in a slot including the location of the physical adapter

#### Model

Model, which is the same as the product name

#### Port

Displays the port number of each adapter port. Provides address and interconnect details.

Address | Displays the MAC address and WWPN of each adapter port
Interconnect | The corresponding interconnect and downlink port

The Ports panel does not display information about rack servers.

## Remote Support

Once remote support is enabled, you can configure and edit the remote support settings and collect remote support data.

#### Status

Enabled or will say Remote Support is not enabled on the appliance if you have not enabled remote support.

#### Contacts

Name | The name of the remote support contact
Type | Primary or secondary
Email | Email of contact
Phone number | Phone number of contact

#### Channel Partners

Name | Name of channel partner or partners
Type | Reseller or support
City | City location
Country | Country location

#### Remote Support Data

Status | Status of the data collection such as completed, submitted or error
ID | Identifier for the data collection
Collection date | The date and time the data was collected
Type | Basic or active health collection Active health is transmitted every 7 days. Basic data is transmitted every 30 days.

#### More information

Collect remote support data for servers
About data collection
Settings: Remote support

## Add Server Hardware

Rack servers are the only type of server hardware added via the Server Hardware screen. To add a server blade, see Add server hardware to managed enclosures.

| IMPORTANT: Forcibly adding a rack server that is managed by another appliance for monitoring will make it inaccessible to the other management system.

#### iLO IP address or host name

iLO IP address or host name of the rack server's iLO management processor.

The imported rack server is named using the iLO subsystem name.

#### Add server hardware as

Select whether you want to manage or monitor the rack server.

Managed | You can apply configurations, deploy server profiles, analyze operation status, collect statistics, and alert users to specific conditions.
Monitored | You can view hardware for inventory and status information only.
| NOTE: The HPE OneView Standard license is automatically selected.

#### User name

iLO login name of an account with administer user accounts privilege

Default value: | `Administrator`

#### Password

iLO password

#### Licensing

Select a license type for the server hardware. Server license types are dictated by the license policy of the enclosure that contains them. If the server hardware has an embedded license, the appliance applies that license to it, regardless of the license type you choose or the license policy of the enclosure in which it resides. See About licensing and About rack mount server licensing to learn more.

OneView | Contains both a OneView license and an iLO Advanced license. Applies a OneView and a permanent iLO Advanced license to the server hardware.
OneView w/o iLO | Contains only a OneView license. Applies a OneView license to the server hardware. To apply an existing iLO license, you have to add the license on the server hardware iLO which is not a part of a .OneView license

#### More information

Standard UI buttons
Server Hardware

## Edit a rack server

#### Maximum power

Maximum power this device can consume in watts.

#### More information

Adding a server
Edit a rack server
Standard UI buttons
Server Hardware

prev | up | next
Enabling health monitoring for legacy servers | home | Edit a rack server

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP