Networks > Create multiple Ethernet networks using a single POST operation |  | next

# Create multiple Ethernet networks using a single `POST` operation

When you create multiple Ethernet networks, you must specify VLAN IDs in the range 2–4094.

To learn more about tagged networks, see About networks.

| NOTE: When you add multiple Ethernet networks at once, you can only specify `Tagged` for the `ethernetNetworkType` attribute.

### Prerequisites

- Minimum required session ID privileges: Network administrator

Creating multiple Ethernet networks using a single `POST` operation using REST APIs
`POST /rest/ethernet-networks/bulk`

| NOTE: The `connectionTemplateUri` attribute must be set to `null`.

prev | up | next
Create an Ethernet network | home | Create a Fibre Channel network

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP