Interconnects > Reset loop and pause flood protection |  | next

# Reset loop and pause flood protection

You can reset the loop and pause flood protection for an interconnect from the appliance. You might want to do this after resolving a network loop or pause flood condition.

For more information on loop and pause flood protection, see About loop protection and About pause flood protection.

Prerequisites

- Infrastructure administrator or Network administrator

- The interconnect is managed

Resetting loop and pause flood protection

1. From the main menu, select Interconnects.

2. In the master pane, select the interconnect for which you want to reset the loop and pause flood protection.

3. Select Actions→Reset loop and pause flood protection.

   | NOTE: The Reset action starts immediately, confirmation is not required.

4. If the activity is successful, the activity displays a green status in the Notifications area. If not, follow the proposed resolution listed under Details in the Notifications area.

See also

- Interconnects

prev | up | next
Replace an interconnect | home | View data transfer statistics for uplink and downlink ports

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP