Server Hardware > Reassign the server profile to a server blade previously removed from an enclosure |  | next

# Reassign the server profile to a server blade previously removed from an enclosure

When you reinsert a server blade into the same bay, the server profile is reassociated with it and a task notification is created. But, if you reinsert a server blade into a different bay, the server profile associated with that server blade has a task error message stating that the server blade has been moved to a new location. To resolve this issue, either reassign the server profile to the server blade in the new location, or move the server blade to the original bay.

### Prerequisites

- Minimum required session ID privileges: Server administrator

Reassigning the server profile to a server blade previously removed from an enclosure using REST APIs
Get the server blade that was reinserted into a different bay. `GET /rest/server-hardware?filter="state='AddedWithErrors'"` Get the server profile URI that was associated with the server blade. `GET /rest/tasks?filter="associatedResourceUri='`{server blade URI}`'"` Get the server profile associated with the server blade. `GET /rest/server-profiles/`{id}`` Add the correct server hardware URI to the server profile. Update the server profile. `POST /rest/server-profiles`

prev | up | next
Power on or power off server hardware | home | Read a rack server

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP