Switches > Remove a switch |  | next

# Remove a switch

The Remove action is available only for switches that are migrated from HPE OneView version 1.`x`. Logical switch groups and logical switches are available only from HPE OneView version 2.0 and later. Migrated switches do not have an associated logical switch. These switches are not known to HPE OneView until they are explicitly added by creating a logical switch.

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Removing a switch

1. From the main menu, select Switches, and select the switch to remove.

2. Select Actions→Remove.

3. Verify that the switch has been removed from the Switches screen.

See also

- About top-of-rack switches

prev | up | next
Refresh a switch | home | Troubleshooting

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP