Firmware Bundles > Establish a firmware baseline for your managed devices |  | next

# Establish a firmware baseline for your managed devices

Use an SPP to establish a firmware baseline for your environment. The appliance attempts to automatically update the firmware while the resource is being added to the appliance.

Enclosure power supplies and fans | Firmware is updated when you apply the SPP to enclosures.
Interconnects | Firmware is updated when you assign an SPP to the logical interconnect configuration.
Server blades or rack mount servers | Server and iLO firmware is updated when you apply a server profile.

| IMPORTANT: To ensure optimal system health and performance, keep the firmware repository updated with the latest SPPs, and regularly assign those SPPs as baselines to your enclosure groups or devices.

See also

- Firmware Bundles

prev | up | next
Create a custom SPP | home | Remove a firmware bundle from the firmware bundle repository

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP