Power Delivery Devices > Add a non-iPDU power delivery device |  | next

# Add a non-iPDU power delivery device

Power delivery devices that the appliance cannot discover are considered unmanaged. You must provide configuration information about them before the appliance can add and analyze them. Entering configuration information about these unmanaged power delivery devices ensures more accurate analysis of power capacity, power consumption, and redundancy.

To add a description of a power delivery device that is not an iPDU under the appliance management, add the attributes manually.

### Prerequisites

- Minimum required session ID privileges: Server administrator

Adding a non-iPDU power delivery device using REST APIs
`POST /rest/power-devices`

prev | up | next
Control power to a power delivery device outlet | home | Read a power device

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP