Logical Interconnects > Update logical interconnect SNMP settings |  | next

# Update logical interconnect SNMP settings

To update logical interconnect SNMP settings, perform a `PUT` operation to reapply all of the logical interconnect SNMP settings attributes. View the logical interconnect SNMP settings attributes by using a `GET` operation, edit the attributes, and then perform a `PUT` operation using all of the attributes.

### Prerequisites

- Minimum required session ID privileges: Infrastructure administrator

Updating logical interconnect SNMP settings using REST APIs
Select a logical interconnect URI. `GET /rest/logical-interconnects` Using the logical interconnect URI, get the logical interconnect SNMP settings. `GET `{logical interconnect URI}`/snmpConfiguration` Edit the SNMP settings. Update the logical interconnect SNMP settings. `PUT `{logical interconnect URI}`/snmpConfiguration`

prev | up | next
Update internal networks on a logical interconnect | home | Update a logical interconnect Link Aggregation Control Protocol (LACP) timer

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP