Enclosures > Bring an unmanaged c7000 enclosure under management |  | next

# Bring an unmanaged c7000 enclosure under management

An enclosure might become unmanaged if the firmware is invalid or if the enclosure was discovered when adding an HPE Intelligent Power Distribution Unit (HPE iPDU). To update the firmware and bring an unmanaged enclosure under management, see Bring an unmanaged enclosure with invalid firmware under management.

Prerequisites

- Required privileges: Infrastructure administrator or Server administrator

Bringing an unmanaged enclosure discovered via iPDU under management

If an enclosure is discovered via an iPDU, that enclosure is considered unmanaged until the OA credentials are added. You will be able to add the OA credentials when you add the enclosure.

- Add the enclosure.

prev | up | next
Add server hardware to managed enclosures | home | Claim a c7000 enclosure currently being managed by another management system

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP