Interconnects > Replace an interconnect |  | next

# Replace an interconnect

Configuration settings are applied to a bay and not to individual interconnects. When replacing an interconnect, you do not need to configure the new interconnect if you are installing it in the same bay.

Logical interconnect groups are associated with bays only if there are interconnects configured for the bay.

To add a new interconnect in a different bay, edit the logical interconnect group that is associated with the bay in the enclosure group.

See also

- Interconnects

prev | up | next
Reapply interconnect configuration | home | Reset loop and pause flood protection

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP