Logical Interconnects > Delete an uplink set |  | next

# Delete an uplink set

Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

Deleting an uplink set

1. From the main menu, select Logical Interconnects, and then select the logical interconnect from which you want to delete an uplink set.

2. Click the Edit icon to edit the uplink sets.

3. Click the Delete icon of the uplink set you want to delete in the graphical view.

4. Confirm you want to delete the uplink set and click Yes, delete.

5. Verify the uplink set no longer appears in the Logical Interconnects view and click OK.

See also

- Logical Interconnects (top of chapter)

prev | up | next
Configure a port to monitor network traffic | home | Edit a logical interconnect

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP