Server Hardware > Remove a rack server from management |  | next

# Remove a rack server from management

Use this procedure to remove an HPE ProLiant rack server from management.

| NOTE: To remove a server blade from management, you must physically remove the server blade. See Remove a server from an existing enclosure .

Removing a server from management removes its alerts, activities, and associations.

You cannot remove a server that is hosting an active server profile. You must delete the server profile from the server, and then remove the server from management.

If the appliance cannot contact the server during the remove operation, a message alerts you about manual cleanup tasks.

Prerequisites

- Required privileges: Infrastructure administrator or Server administrator

Removing a rack server

1. From the main menu, select Server Hardware.

2. In the master pane, select the rack server you want to remove.

3. Select Actions→Remove.

4. Review the confirmation message, if any, and click Yes, remove to remove the rack server.

5. Verify that the rack server has been removed in the master pane.

See also

- Server Hardware

prev | up | next
Collect remote support data for servers | home | Claim a server currently being managed by another management system

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP