Logical Interconnects > Set up logical interconnect port monitoring |  | next

# Set up logical interconnect port monitoring

For analysis, you can use port monitoring to duplicate and direct network traffic to one logical interconnect port from up to 16 physical servers.

### Prerequisites

- Minimum required session ID privileges: Network administrator

Set up logical interconnect port monitoring using REST APIs
Select the logical interconnect URI. `GET /rest/logical-interconnects` Using the logical interconnect URI, get the current port monitoring information. `GET `{logical interconnect URI}`/port-monitor` Enable port monitoring and add the list of ports you want to monitor. `PUT `{logical interconnect URI}`/port-monitor`

prev | up | next
Reapply a logical interconnect group to bring a logical interconnect into compliance | home | Update internal networks on a logical interconnect

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP