Logical Interconnect Groups > Enable or disable LLDP tagging using REST APIs |  | next

# Enable or disable LLDP tagging using REST APIs

Enabling or disabling the `enableTaggedLldp` parameter determines the LLDP management address TLV of LLDP frames sent out by an interconnect.

## Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

- Minimum required Virtual Connect firmware version: 4.45

## Enabling LLDP tagging using REST APIs

1. Select a logical interconnect group URI.

   `GET /rest/logical-interconnect-groups`

2. Get the logical interconnect group using the URI from step 1.

   `GET /rest/logical-interconnect-groups/`{id}``

3. Set `enableTaggedLldp` to `true`.

4. Update the logical interconnect group.

   `PUT /rest/logical-interconnect-groups/`{id}``

## Disabling LLDP tagging using REST APIs

1. Select a logical interconnect group URI.

   `GET /rest/logical-interconnect-groups`

2. Get the logical interconnect group using the URI from step 1.

   `GET /rest/logical-interconnect-groups/`{id}``

3. Set `enableTaggedLldp` to `false`.

4. Update the logical interconnect group.

   `PUT /rest/logical-interconnect-groups/`{id}``

#### More information

About Link Layer Discovery Protocol (LLDP) tagging

prev | up | next
Update logical interconnect group SNMP settings | home | Enable or disable enhanced TLV support using REST APIs

Copyright © 2013-2016 Hewlett Packard Enterprise Development LP