Networks > Create networks |  | next

# Create networks

Create networks to define connections that route data across the IT infrastructure. You can create a single Ethernet, Fibre Channel, or FCoE network or multiple, tagged Ethernet networks at one time.

For more information about networks and how to use them, see About networks.

Prerequisites

- Minimum required privileges: Network administrator

Creating networks

1. From the main menu, select Networks, and then do one of the following:

   - Click + Create network in the master pane.

   - Select Actions→Create.

   | NOTE: The Actions menu is not displayed until you create at least one network.

2. Enter the data requested on the screen. See Create or Edit a network screen details for more information.

   | NOTE: To create multiple, tagged Ethernet networks, type in a set of values or a range of values in the VLAN ID field. For example: `113, 114, 200–300`.

3. Click Create to complete the action or click Create + to create another network.

4. Verify that the network or networks were created in the master pane.

### More information

About networks
Quick Start: Initial configuration of resources in HPE OneView

prev | up | next
Networks screen details | home | Edit network configuration settings

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP