Enclosures > BIOS acknowledgment for in-service migration |  | next

# BIOS acknowledgment for in-service migration

In Virtual Connect Manager, administrators can configure specific boot settings (such as PXE or SAN boot) for profile connections while leaving the default `USE-BIOS` setting in place on other connections in the same profile. After in-service migration, the server continues to boot based on the configured boot settings. However, the first time the server is rebooted after in-service migration, any connection on the profile configured to `USE-BIOS` is converted to `not bootable` to match HPE OneView conventions.

#### More information

Migrate a c7000 enclosure currently managed by VCM
About migration acknowledgments

prev | up | next
Redundant hardware and software configuration acknowledgment for in-service migration | home | SR-IOV acknowledgment for in-service migration

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP