Server Profiles > Server Profiles status icon definitions |  | next

# Server Profiles status icon definitions

Icon | Health status | Description
--- | --- | ---
| Unknown | The `Unknown` status occurs when a server profile is in the process of being created and applied to the server hardware.
| OK | The server profile status is `OK` when a server profile is successfully created and applied to the server hardware.
| Warning | The server profile status can be in a `Warning` condition when noncritical issues that require attention are detected, such as: The maximum bandwidth for the network is reduced below the bandwidth requested in the server profile.
| Error | The server profile status can be in an `Error` condition when: The server profile cannot be successfully applied to the server hardware. A network that is being used by the server profile is deleted, and the requested network connections cannot be created or cannot be deployed.
| Applying Change | The `Applying Change` icon can be overlaid in combination with the `Unknown`, `OK`, or `Warning` status icons while a task is running on the resource. For example, when a change is being applied to an existing server profile, its status is `OK` + `Applying Change`, displays as: When a server profile is in the `Applying Change` state, do not reboot the server hardware.

See also

- Server Profiles

prev | up | next
Server Profiles screen details | home | Create and apply a server profile

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP