Power Delivery Devices > Add a power connection |  | next

# Add a power connection

You can add and edit the power supply connections to power delivery devices. The Add connection dialog box displays the power supplies connected to the device; for example, an HPE BladeSystem c7000 Enclosure has six power supplies. The changes you make on this screen are saved when you save the rack configuration.

If HPE Power Discovery Services detects a connection, the device name is populated automatically.

The Add connections dialog box displays leaf power delivery devices in the rack that are compatible with the device. Power delivery devices that are in use by other devices are not displayed.

Prerequisites

- Required privileges: Infrastructure administrator or Server administrator

Adding a power connection

1. From the main menu, select Power Delivery Devices, and do one of the following:

   - In the master pane, select the power delivery device to which you want to add a connection and select Actions→Edit.

   - Hover your pointer in the details pane and click the Edit icon.

2. Under Power Connections, click Add connections.

3. In the Add connections dialog box, select a device from the list (press and hold Ctrl to select multiple devices) and click Add to add a connection between that device and the power delivery device, or click Add + to add another connection.

4. When you are finished adding connections, click OK.

5. Verify that the power connection has been added in the details pane.

See also

- About power delivery devices

- Power Delivery Devices

- Return to Quick Start: Initial configuration

prev | up | next
Add a power delivery device | home | Filter power delivery devices

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP