Interconnects > Reapply interconnect configuration |  | next

# Reapply interconnect configuration

You can reapply the configuration settings of a physical interconnect from the appliance using the reapply configuration feature. You may want to do this after replacing an interconnect, after a connection loss, or if interconnect configuration fails.

Prerequisites

- Infrastructure administrator or Network administrator

- The interconnect is managed

Reapplying interconnect configuration

1. From the main menu, select Interconnects.

2. In the master pane, select the interconnect for which you want to reapply the configuration.

3. Select Actions→Reapply configuration.

4. If server profiles are using the interconnect, a dialog box displays warning that network connectivity for the server profiles using the interconnect may be disrupted. Click Yes, reapply if you want to continue.

5. If the activity is successful, the activity displays a green status in the Notifications area. If not, follow the proposed resolution listed under Details in the Notifications area.

See also

- About interconnects

- Interconnects

prev | up | next
Enable or disable uplink or downlink ports on an interconnect | home | Replace an interconnect

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP