Logical Interconnect Groups > Copy a logical interconnect group |  | next

# Copy a logical interconnect group

You can copy the existing settings of a logical interconnect group to a new logical interconnect group.

## Prerequisites

- Required privileges: Infrastructure administrator or Network administrator

## Copying a logical interconnect group

1. From the main menu, select Logical Interconnect Groups and select the interconnect group to copy.

2. Select Actions→Copy.

3. Enter the name of the new logical interconnect group.

4. Click OK.

   HPE OneView uses the existing logical interconnect group and creates a new logical interconnect group. The new logical interconnect group is not associated with any enclosure groups or logical interconnects.

5. Verify that the new logical interconnect group appears in the master pane.

#### More information

About copying a logical interconnect group

prev | up | next
Delete a logical interconnect group | home | Enable or disable Link Layer Discovery Protocol (LLDP) tagging

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP