|  | next

# Logical Interconnect Groups

A logical interconnect group acts as a recipe for creating a logical interconnect representing the available networks, uplink sets, and interconnect settings for a set of physical interconnects in a single enclosure.

I want to ... Create a logical interconnect group Edit a logical interconnect group Delete a logical interconnect group Edit internal networks Copy a logical interconnect group Enable or disable Link Layer Discovery Protocol (LLDP) tagging Enable or disable enhanced type-length-value (TLV) settings Manage SNMP access for c7000 enclosures Manage SNMP trap destinations Manage the frequency of control messages through the LACP timer See more tasks | Learn more About logical interconnect groups About the logical interconnect group graphical interface About multiple logical interconnect groups in an enclosure group About uplink sets in a logical interconnect group About Link Layer Discovery Protocol (LLDP) tagging About copying a logical interconnect group About Quality of Service for network traffic About SNMP settings Logical Interconnect Groups screen details

prev |  | next
View the general configuration of a logical interconnect | home | About logical interconnect groups

Copyright © 2013, 2016 Hewlett Packard Enterprise Development LP